IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2020-04-08T08:57:28"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637219258489938086 | last modified 637219258489938086
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Modul Q 900 Project" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "Modul Q 900 Project" | DIRECTIONSOURCE | 1 occurrence | description "LED ceiling luminaire for suspended mounting, closed luminaire housing, cover on top made of plastic, high gloss white (RAL 9016), diffuser panel made of acrylic glass with conical indentations for directing the light and reducing glare, 900 × 900 mm, 6 mm thick, with rounded corners and all round chamfer, both sides matt, non-glare in accordance with DIN EN 12464-1, suitable for workplace lighting, light distribution approx. 98 % direct beam, wide beam, version for 24 V DC, please order canopy with supply and operating devices and suspension sets separately according to your individual mounting situation. (canopy with operating devices, switchable: 546-844, dimmable 1-10 V: 546-843, dimmable DALI/switchDIM: 546-735, dimmable CASAMBI: 549-720 / suspension kit Modul Q Project, length 2 m: 546-767, length 4 m: 546-768)"

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "Not specified" (IFCTEXT)
    Product group = ["MODUL Q PROJECT", "Suspended luminaire"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "Modul Q 900 Project" (IFCTEXT)
    Article number = "546-834" (IFCTEXT)
    Uld creation date = "04.08.2020 00:00:00" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Pendulum length = 100. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 59. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"Pendant"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "NIMBUS" (IFCTEXT)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 59. (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Lamp lifetime = 1000. (IFCREAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 1. (IFCREAL)
    Luminous flux = 6475. (IFCNUMERICMEASURE) [LUMEN]
    Socket = "-" (IFCTEXT)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 85 (IFCINTEGER)
    ColorTemperature = 3000. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 6475. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 59. (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)