IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2020-03-26T16:08:41"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637208321212900592 | last modified 637208321212900592
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Modul Q 64" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "Modul Q 64" | DIRECTIONSOURCE | 1 occurrence | description "Ultra-flat LED ceiling luminaire with 10 mm thickness only, light distribution approx. 98 % direct beam, wide beam, additional ceiling lighting and very even, almost floor-to-ceiling illumination of walls by secondary light, flexible application by means of magnetic attachment, version for 24 volts DC, external converter required, please order mounting set separately according to your individual mounting situation (luminaire with ceiling ring for direct mounting: 004-180, luminaire with bracket for cavity mounting: 004-191)."

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "White" (IFCTEXT)
    Product group = ["MODUL Q", "Ceiling luminaire"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "Modul Q 64" (IFCTEXT)
    Article number = "554-469" (IFCTEXT)
    Uld creation date = "26.03.2020 15:08:41" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Recessed depth = 0. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 10.5 (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"SurfaceMounted"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "NIMBUS" (IFCTEXT)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 10.5 (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Lamp lifetime = 1000. (IFCREAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 1. (IFCREAL)
    Luminous flux = 1350. (IFCNUMERICMEASURE) [LUMEN]
    Socket = "-" (IFCTEXT)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 90 (IFCINTEGER)
    ColorTemperature = 4000. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 1350. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 10.5 (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)