IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2020-03-26T15:57:38"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637208314585927940 | last modified 637208314585927940
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Modul L 196 Sequence 2" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "Modul L 196 Sequence 2" | DIRECTIONSOURCE | 1 occurrence | description "Extremely slim, height-adjustable LED suspended luminaire for wide-area room lighting for offices and workplaces, sequence of two luminaire modules L 196, mechanical and electrical link by a connector element,support made of anodised aluminium, diffuser made of matt acrylic glass, 384 conical indentations for directing light and reducing glare, suitable for workplace lighting in accordance with DIN EN 12464-1, approx. 98 % direct beam, set including 1 module connector made of aluminium, powder coated white and 3 stainless steel suspension cables, adjustable from 100 to 1500 mm, version for 24 volts DC, please order canopy with supply and operating devices or external converter separately (canopy with operating devices, switchable: 545-864, dimmable 1-10 V: 545-865, dimmable DALI/switchDIM: 545-866, external converter for cavity mounting: 551-401)."

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "Not specified" (IFCTEXT)
    Product group = ["MODUL L", "Suspended luminaire"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "Modul L 196 Sequence 2" (IFCTEXT)
    Article number = "545-852" (IFCTEXT)
    Uld creation date = "26.03.2020 14:57:38" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Pendulum length = 100. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 47. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"Pendant"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "NIMBUS" (IFCTEXT)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 47. (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Lamp lifetime = 1000. (IFCREAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 0.92744157247842784 (IFCREAL)
    Luminous flux = 6600. (IFCNUMERICMEASURE) [LUMEN]
    Socket = "-" (IFCTEXT)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 85 (IFCINTEGER)
    ColorTemperature = 4000. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 6600. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 47. (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)