IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2022-02-02T09:24:41"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.2.1.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.2.1.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637793870819609754 | last modified 637793870819609754
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LP Lounge Santos Rosewood / White" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "LP Lounge Santos Rosewood / White" | DIRECTIONSOURCE | 1 occurrence | description "Acoustically effective pendant luminaire with body made of shaped wood, available in different high-quality types of wood, embossed front fleece, diameter 696 mm, canopy with driver and integrated mechanical clamps for height adjustment of suspension cables, sound absorption class B, 8 Bartenbach lenses placed in the acoustic pad, effective indirect light component integrated in the shaped wood, light distribution approx. 49 % direct and 51 % indirect beam, direct light component with narrow beam, indirect light component glare-free by means of conical indentations, colour temperature adjustable 2700-4000 K, CRI > 90, controllable and dimmable via sensors or Bluetooth® wireless technology."

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "Not specified" (IFCTEXT)
    Product group = ["LIGHTING PAD LOUNGE", "sound-absorbing acoustic luminaire"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "LP Lounge Santos Rosewood / White" (IFCTEXT)
    Article number = "560-665" (IFCTEXT)
    Uld creation date = "02.02.2022 00:00:00" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Pendulum length = 100. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 54. (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"Pendant"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "Nimbus" (IFCTEXT)
    NumberOfSources = 9 (IFCINTEGER)
    TotalWattage = 3.25 (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 9 objects (9 IFCFLOWTERMINAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 1. (IFCREAL)
    Luminous flux = 212.5 (IFCNUMERICMEASURE) [LUMEN]
  Pset_LampTypeCommon | properties | on 8 objects (8 IFCFLOWTERMINAL)
    ColorRenderingIndex = 90 (IFCINTEGER)
    ColorTemperature = 3114. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 212.5 (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 3.25 (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 90 (IFCINTEGER)
    ColorTemperature = 3114. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 1800. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 28. (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)