IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2020-03-26T15:56:03"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.1.27.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637208313632436223 | last modified 637208313632436223
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Rim R 9" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "Rim R 9" | DIRECTIONSOURCE | 1 occurrence | description "LED ceiling luminaire, continuously tiltable up to approx. 90° and rotatable up to approx. 350°, approx. 95 % direct beam, wide beam, the effect of wall illumination by means of secondary lighting is largely maintained even with the manoeuvrability of the luminaire head, version with integrated converter for connection to 230 volts ceiling outlets, body available in various surface finishes (brilliant white, frosted silver anodised, brilliant polished chrome, matt titanium grey anodised, matt gold anodised, matt black anodised), central cover brilliant white."

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "Not specified" (IFCTEXT)
    Product group = ["Rim R", "rotatable and tiltable"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "Rim R 9" (IFCTEXT)
    Article number = "545-673" (IFCTEXT)
    Uld creation date = "26.03.2020 14:56:03" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Recessed depth = 0. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 4.2 (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"SurfaceMounted"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "NIMBUS" (IFCTEXT)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 4.2 (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Lamp lifetime = 1000. (IFCREAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 0.95916718970531389 (IFCREAL)
    Luminous flux = 190. (IFCNUMERICMEASURE) [LUMEN]
    Socket = "-" (IFCTEXT)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 90 (IFCINTEGER)
    ColorTemperature = 2700. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 190. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 4.2 (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)