IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2021-01-15T11:50:31"
Preprocessor: "Xbim File Processor version 4.0.0.0"
Originating system: "Xbim version 4.0.0.0"
Application: "DIALux" version "1.1.29.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
Application: "DIALux" identifier "Evo" by Organization "DIALux-Team"

People and organizations
  Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany")
  Person (no name given) of Organization "DIAL GmbH"
  Owner history of Person (no name given) of Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | application "DIALux" version "1.1.29.0" identifier "Uld2IFC Export" by Organization "DIAL GmbH" (postal address: "Bahnhofsallee 18", "Lüdenscheid", "NRW", "Germany") | state READWRITE | change ADDED | created 637463046314440262 | last modified 637463046314440262
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change MODIFIED | created 0 (1970-01-01T00:00:00Z)
  Owner history of Person (no name given) of Organization "DIAL GmbH" | application "DIALux" identifier "Evo" by Organization "DIALux-Team" | change ADDED | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "DIALux"
  IFCBUILDING "Default Building"
    contains 1 element
      1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Rahmenlos" | material: layers ((no material) 10.) | property sets: Marketing Information, General Information, Mounting Information, Pset_ElectricalDeviceCommon, Pset_LightFixtureTypeCommon

Types
  IFCLIGHTFIXTURETYPE "Rahmenlos" | DIRECTIONSOURCE | 1 occurrence | description "Frameless LED luminaire for recessed ceiling mounting with aluminium housing and matt glass cover, installation kit for flush mounting included, light emission 100 % direct beam, ultra-shallow mounting depth, version for 24 V DC, external converter required."

Property sets
  Marketing Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Emergency lighting possible = FALSE (IFCLOGICAL)
    Housing color = "Not specified" (IFCTEXT)
    Product group = ["Rahmenlos", "Recessed ceiling-mounted luminaire"] (IFCTEXT)
  General Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article name = "Rahmenlos" (IFCTEXT)
    Article number = "010-463" (IFCTEXT)
    Uld creation date = "15.01.2021 10:50:31" (IFCLABEL)
  Mounting Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Recessed depth = 0. (IFCNUMERICMEASURE) [CENTI METRE]
  Pset_ElectricalDeviceCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ElectricalDeviceNominalPower = 7.1 (IFCPOWERMEASURE) [WATT]
  Pset_LightFixtureTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    LightFixtureMountingType in {"Recessed"} (IFCLABEL)
    LightFixturePlacingType in {"Ceiling"} (IFCLABEL)
    ManufacturersSpecificInformation = "NIMBUS" (IFCTEXT)
    NumberOfSources = 1 (IFCINTEGER)
    TotalWattage = 7.1 (IFCPOWERMEASURE) [WATT]
  Photometric Information | properties | on 1 object (1 IFCFLOWTERMINAL)
    Lamp lifetime = 1000. (IFCREAL)
    Lamp names = "LED" (IFCTEXT)
    Light output ratio = 1. (IFCREAL)
    Luminous flux = 580. (IFCNUMERICMEASURE) [LUMEN]
    Socket = "-" (IFCTEXT)
  Pset_LampTypeCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    ColorRenderingIndex = 90 (IFCINTEGER)
    ColorTemperature = 2700. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [KELVIN]
    ContributedLuminousFlux = 580. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    LightEmitterNominalPower = 7.1 (IFCPOWERMEASURE) [WATT]
    Spectrum (ifcpropertytablevalue)